<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<packages>
<package name=".2MMBGA20">
</package>
<package name="SOIC-8">
</package>
<package name="CC3100MOD">
</package>
<package name="BSH103">
</package>
<package name="LTV-816S">
</package>
<package name="MDB-PLUG">
</package>
<package name="MDB-SOCKET">
</package>
<package name="WLCSP-20_2.0X1.9X0.6">
</package>
<package name="RFANT5220110A2T">
</package>
<package name="AC0201FR-07100KL">
</package>
<package name="RC0402FR-0710KL">
</package>
<package name="YAG1954CT-ND">
</package>
<package name="RC0603FR-07330RL">
</package>
<package name="IFX27001">
</package>
<package name="PN7120">
</package>
<package name="5031821852">
</package>
<package name="C1206C106J9RACTU">
</package>
<package name="XRCGB27M120F3M10R0">
</package>
<package name="E_BUTTON(TL3315NF160Q)">
<description>Momentary N.O. Switch (TL3315NF160Q)</description>
</package>
<package name="MAX175">
<description>Synchronous Step-Down DC-DC Converter, 60V, 1A, Ultra-Small, High-Efficienty</description>
</package>
<package name="SRR1260">
<description>Bourns SRR1260 inductors</description>
</package>
<package name="SRR1260-150M">
</package>
<package name="12PADS">
</package>
<package name="OWL">
</package>
</packages>
<symbols>
<symbol name="KL02Z32CAF4R">
<pin name="E4"/>
<pin name="E3"/>
<pin name="E2"/>
<pin name="E1"/>
<pin name="D4"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="C1"/>
<pin name="C2"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="B1"/>
<pin name="D3"/>
<pin name="D2"/>
<pin name="D1"/>
<pin name="C4"/>
<pin name="C3"/>
</symbol>
<symbol name="SI8420BB-D-IS">
<pin name="A2"/>
<pin name="GND1"/>
<pin name="A1"/>
<pin name="VDD1"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="GND2"/>
<pin name="VDD2"/>
</symbol>
<symbol name="CC3100MOD">
<pin name="VBAT_DCDC_DIG_IO"/>
<pin name="VBAT_DCDC_ANA"/>
<pin name="VBAT_DCDC_PA"/>
<pin name="NRESET"/>
<pin name="HOST_INTR"/>
<pin name="FORCE_AP"/>
<pin name="RESERVED"/>
<pin name="GND"/>
<pin name="TCXO_EN/SOP2"/>
<pin name="NHIB"/>
<pin name="SPI_CLK"/>
<pin name="SPI_DIN"/>
<pin name="SPI_DOUT"/>
<pin name="SPI_NCS"/>
<pin name="RF_BG"/>
<pin name="UART1_TX"/>
<pin name="UART1_RX"/>
<pin name="UART1_NRTS"/>
<pin name="UART1_NCTS"/>
<pin name="TP1"/>
<pin name="TP2"/>
<pin name="TP3"/>
<pin name="TP4"/>
</symbol>
<symbol name="BSH103">
<pin name="S"/>
<pin name="D"/>
<pin name="G"/>
</symbol>
<symbol name="LTV-816S">
<pin name="CATHODE"/>
<pin name="ANODE"/>
<pin name="EMITTER"/>
<pin name="COLLECTOR"/>
</symbol>
<symbol name="MDB-PLUG">
<pin name="DATA_GND"/>
<pin name="TX"/>
<pin name="RX"/>
<pin name="24V+"/>
<pin name="PWR_GND"/>
<pin name="P$1"/>
</symbol>
<symbol name="MDB-SOCKET">
<pin name="RX"/>
<pin name="TX"/>
<pin name="DATA_GND"/>
<pin name="P$4"/>
<pin name="PWR_GND"/>
<pin name="24V"/>
</symbol>
<symbol name="MKL02Z32CAF4R">
<pin name="PTA12"/>
<pin name="PTB13_2"/>
<pin name="PTA0"/>
<pin name="PTA1"/>
<pin name="EPAD_2" direction="pas"/>
<pin name="PTB3"/>
<pin name="PTB5"/>
<pin name="PTA2"/>
<pin name="VDDVREFH" direction="pwr"/>
<pin name="EPAD_3" direction="pas"/>
<pin name="PTA9"/>
<pin name="PTB4"/>
<pin name="VSSVREFL" direction="pwr"/>
<pin name="PTA3"/>
<pin name="EPAD_4" direction="pas"/>
<pin name="PTA8"/>
<pin name="PTB2"/>
<pin name="PTB13"/>
<pin name="PTA4"/>
<pin name="EPAD" direction="pas"/>
</symbol>
<symbol name="RFANT5220110A2T">
<pin name="RF" direction="pas"/>
</symbol>
<symbol name="RESISTOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="IFX27001">
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="pas"/>
<pin name="IN" direction="pas"/>
</symbol>
<symbol name="PN7120">
<pin name="CLK_REQ" direction="pas"/>
<pin name="XTAL2" direction="pas"/>
<pin name="XTAL1" direction="pas"/>
<pin name="I2C_SCL" direction="pas"/>
<pin name="I2C_ADR0" direction="pas"/>
<pin name="I2C_SDA" direction="pas"/>
<pin name="IRQ" direction="pas"/>
<pin name="BOOST_CTRL" direction="pas"/>
<pin name="RXP" direction="pas"/>
<pin name="RXN" direction="pas"/>
<pin name="TX1" direction="pas"/>
<pin name="TX2" direction="pas"/>
<pin name="ANT2" direction="pas"/>
<pin name="ANT1" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VDD" direction="pas"/>
<pin name="VBAT" direction="pas"/>
<pin name="VEN" direction="pas"/>
<pin name="VDD(MID)" direction="pas"/>
<pin name="VDD(TX)" direction="pas"/>
<pin name="VSS(TX)" direction="pas"/>
</symbol>
<symbol name="5031821852">
<pin name="X"/>
<pin name="CS"/>
<pin name="DI"/>
<pin name="VDD"/>
<pin name="SCLK"/>
<pin name="VSS"/>
<pin name="DO"/>
<pin name="X8"/>
</symbol>
<symbol name="C1206C106J9RACTU">
<pin name="RIGHT"/>
<pin name="LEFT"/>
</symbol>
<symbol name="CRYSTAL">
<pin name="L"/>
<pin name="R"/>
</symbol>
<symbol name="SWITCH">
<pin name="A" direction="nc"/>
<pin name="B" direction="nc"/>
</symbol>
<symbol name="MAX17502">
<pin name="PGND"/>
<pin name="VIN"/>
<pin name="EN"/>
<pin name="VCC"/>
<pin name="FB"/>
<pin name="SS"/>
<pin name="NC"/>
<pin name="NRES"/>
<pin name="GND"/>
<pin name="LX"/>
</symbol>
<symbol name="INDUCTOR">
<pin name="P2"/>
<pin name="P1"/>
</symbol>
<symbol name="12-PIN2.54MM">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
<pin name="12"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="KL02Z32CAF4R">
<gates>
<gate name="G$1" symbol="KL02Z32CAF4R"/>
</gates>
<devices>
<device name="" package=".2MMBGA20">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="B3" pad="B3"/>
<connect gate="G$1" pin="B4" pad="B4"/>
<connect gate="G$1" pin="C1" pad="C1"/>
<connect gate="G$1" pin="C2" pad="C2"/>
<connect gate="G$1" pin="C3" pad="C3"/>
<connect gate="G$1" pin="C4" pad="C4"/>
<connect gate="G$1" pin="D1" pad="D1"/>
<connect gate="G$1" pin="D2" pad="D2"/>
<connect gate="G$1" pin="D3" pad="D3"/>
<connect gate="G$1" pin="D4" pad="D4"/>
<connect gate="G$1" pin="E1" pad="E1"/>
<connect gate="G$1" pin="E2" pad="E2"/>
<connect gate="G$1" pin="E3" pad="E3"/>
<connect gate="G$1" pin="E4" pad="E4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SI8420BB-D-IS">
<gates>
<gate name="G$1" symbol="SI8420BB-D-IS"/>
</gates>
<devices>
<device name="" package="SOIC-8">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="GND2" pad="GND2"/>
<connect gate="G$1" pin="VDD1" pad="VDD1"/>
<connect gate="G$1" pin="VDD2" pad="VDD2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CC3100MOD">
<gates>
<gate name="G$1" symbol="CC3100MOD"/>
</gates>
<devices>
<device name="" package="CC3100MOD">
<connects>
<connect gate="G$1" pin="FORCE_AP" pad="FORCE_AP"/>
<connect gate="G$1" pin="GND" pad="GND-16 GND-27 GND-28 GND-30 GND-32 GND-38 GND-43 GND-55.1 GND-55.2 GND-55.3 GND-55.4 GND-55.5 GND-56 GND-57 GND-58 GND-59 GND-60 GND-61 GND-62 GND-63 GND1 GND2"/>
<connect gate="G$1" pin="HOST_INTR" pad="HOST_INTR"/>
<connect gate="G$1" pin="NHIB" pad="N_HIB"/>
<connect gate="G$1" pin="NRESET" pad="N-RESET"/>
<connect gate="G$1" pin="RESERVED" pad="RESERVED21-ADD100KPULLDOWN"/>
<connect gate="G$1" pin="RF_BG" pad="RF_BG"/>
<connect gate="G$1" pin="SPI_CLK" pad="HOST_SPI_CLK"/>
<connect gate="G$1" pin="SPI_DIN" pad="HOST_SPI_DIN"/>
<connect gate="G$1" pin="SPI_DOUT" pad="HOST_SPI_DOUT"/>
<connect gate="G$1" pin="SPI_NCS" pad="HOST_SPI_N-CS"/>
<connect gate="G$1" pin="TCXO_EN/SOP2" pad="SOP2(ADD10KPULL)-23"/>
<connect gate="G$1" pin="TP1" pad="TEST_58"/>
<connect gate="G$1" pin="TP2" pad="TEST_59"/>
<connect gate="G$1" pin="TP3" pad="TEST_60"/>
<connect gate="G$1" pin="TP4" pad="TEST_62"/>
<connect gate="G$1" pin="UART1_NCTS" pad="UART1_NCTS"/>
<connect gate="G$1" pin="UART1_NRTS" pad="UART1_NRTS"/>
<connect gate="G$1" pin="UART1_RX" pad="UART1_RX"/>
<connect gate="G$1" pin="UART1_TX" pad="UART1_TX"/>
<connect gate="G$1" pin="VBAT_DCDC_ANA" pad="VBAT-DCDC_ANA"/>
<connect gate="G$1" pin="VBAT_DCDC_DIG_IO" pad="VBAT_DCDC_DIG_IO"/>
<connect gate="G$1" pin="VBAT_DCDC_PA" pad="VBAT_DCDC_PA"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BSH103">
<gates>
<gate name="G$1" symbol="BSH103"/>
</gates>
<devices>
<device name="" package="BSH103">
<connects>
<connect gate="G$1" pin="D" pad="D"/>
<connect gate="G$1" pin="G" pad="G"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTV-816S">
<gates>
<gate name="G$1" symbol="LTV-816S"/>
</gates>
<devices>
<device name="" package="LTV-816S">
<connects>
<connect gate="G$1" pin="ANODE" pad="ANODE"/>
<connect gate="G$1" pin="CATHODE" pad="CATHODE"/>
<connect gate="G$1" pin="COLLECTOR" pad="COLLECTOR"/>
<connect gate="G$1" pin="EMITTER" pad="EMITTER"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MDB_PLUG">
<gates>
<gate name="G$1" symbol="MDB-PLUG"/>
</gates>
<devices>
<device name="" package="MDB-PLUG">
<connects>
<connect gate="G$1" pin="24V+" pad="24V"/>
<connect gate="G$1" pin="DATA_GND" pad="5V-GND"/>
<connect gate="G$1" pin="P$1" pad="NC"/>
<connect gate="G$1" pin="PWR_GND" pad="0V"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MDB_SOCKET">
<gates>
<gate name="G$1" symbol="MDB-SOCKET"/>
</gates>
<devices>
<device name="" package="MDB-SOCKET">
<connects>
<connect gate="G$1" pin="24V" pad="24V"/>
<connect gate="G$1" pin="DATA_GND" pad="DATAGND"/>
<connect gate="G$1" pin="P$4" pad="NC"/>
<connect gate="G$1" pin="PWR_GND" pad="0"/>
<connect gate="G$1" pin="RX" pad="RX"/>
<connect gate="G$1" pin="TX" pad="TX"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MKL02Z32CAF4R" prefix="U">
<gates>
<gate name="A" symbol="MKL02Z32CAF4R"/>
</gates>
<devices>
<device name="" package="WLCSP-20_2.0X1.9X0.6">
<connects>
<connect gate="A" pin="EPAD" pad="D5"/>
<connect gate="A" pin="EPAD_2" pad="A5"/>
<connect gate="A" pin="EPAD_3" pad="B5"/>
<connect gate="A" pin="EPAD_4" pad="C5"/>
<connect gate="A" pin="PTA0" pad="A3"/>
<connect gate="A" pin="PTA1" pad="A4"/>
<connect gate="A" pin="PTA12" pad="A1"/>
<connect gate="A" pin="PTA2" pad="B3"/>
<connect gate="A" pin="PTA3" pad="C4"/>
<connect gate="A" pin="PTA4" pad="D4"/>
<connect gate="A" pin="PTA8" pad="D1"/>
<connect gate="A" pin="PTA9" pad="C1"/>
<connect gate="A" pin="PTB13" pad="D3"/>
<connect gate="A" pin="PTB13_2" pad="A2"/>
<connect gate="A" pin="PTB2" pad="D2"/>
<connect gate="A" pin="PTB3" pad="B1"/>
<connect gate="A" pin="PTB4" pad="C2"/>
<connect gate="A" pin="PTB5" pad="B2"/>
<connect gate="A" pin="VDDVREFH" pad="B4"/>
<connect gate="A" pin="VSSVREFL" pad="C3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CPU" value="ARM Cortex-M0+"/>
<attribute name="FLASHKB" value="32"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="mkl02z32caf4r"/>
<attribute name="MAXFREQUENCY" value="48"/>
<attribute name="PACKAGE" value="WLCSP"/>
<attribute name="PINCOUNT" value="20"/>
<attribute name="SRAMKB" value="4"/>
<attribute name="VENDOR" value="FREESCALE"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RFANT5220110A2T">
<gates>
<gate name="A" symbol="RFANT5220110A2T"/>
</gates>
<devices>
<device name="" package="RFANT5220110A2T">
<connects>
<connect gate="A" pin="RF" pad="RF"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AC0201FR-07100KL">
<gates>
<gate name="A" symbol="RESISTOR"/>
</gates>
<devices>
<device name="" package="AC0201FR-07100KL">
<connects>
<connect gate="A" pin="1" pad="LEFT"/>
<connect gate="A" pin="2" pad="RIGHT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RC0402FR-0710KL">
<gates>
<gate name="A" symbol="RESISTOR"/>
</gates>
<devices>
<device name="" package="RC0402FR-0710KL">
<connects>
<connect gate="A" pin="1" pad="LEFT"/>
<connect gate="A" pin="2" pad="RIGHT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT0603BRD0769R8L">
<gates>
<gate name="A" symbol="RESISTOR"/>
</gates>
<devices>
<device name="" package="YAG1954CT-ND">
<connects>
<connect gate="A" pin="1" pad="D1"/>
<connect gate="A" pin="2" pad="D2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IFX27001">
<gates>
<gate name="A" symbol="IFX27001"/>
</gates>
<devices>
<device name="" package="IFX27001">
<connects>
<connect gate="A" pin="GND" pad="GND"/>
<connect gate="A" pin="IN" pad="IN"/>
<connect gate="A" pin="OUT" pad="3.3V"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="5031821852">
<gates>
<gate name="G$1" symbol="5031821852"/>
</gates>
<devices>
<device name="" package="5031821852">
<connects>
<connect gate="G$1" pin="CS" pad="CD/DAT3-CS"/>
<connect gate="G$1" pin="DI" pad="CMD-DI"/>
<connect gate="G$1" pin="DO" pad="DAT0-DO"/>
<connect gate="G$1" pin="SCLK" pad="CLK-SCLK"/>
<connect gate="G$1" pin="VDD" pad="VDD"/>
<connect gate="G$1" pin="VSS" pad="VSS"/>
<connect gate="G$1" pin="X" pad="DAT2-X"/>
<connect gate="G$1" pin="X8" pad="DAT1-X"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PN7120">
<gates>
<gate name="G$1" symbol="PN7120"/>
</gates>
<devices>
<device name="" package="PN7120">
<connects>
<connect gate="G$1" pin="ANT1" pad="G7"/>
<connect gate="G$1" pin="ANT2" pad="G6"/>
<connect gate="G$1" pin="BOOST_CTRL" pad="D2"/>
<connect gate="G$1" pin="CLK_REQ" pad="A2"/>
<connect gate="G$1" pin="GND" pad="E2"/>
<connect gate="G$1" pin="I2C_ADR0" pad="B2"/>
<connect gate="G$1" pin="I2C_SCL" pad="B1"/>
<connect gate="G$1" pin="I2C_SDA" pad="C1"/>
<connect gate="G$1" pin="IRQ" pad="D1"/>
<connect gate="G$1" pin="RXN" pad="F5"/>
<connect gate="G$1" pin="RXP" pad="F6"/>
<connect gate="G$1" pin="TX1" pad="G3"/>
<connect gate="G$1" pin="TX2" pad="G5"/>
<connect gate="G$1" pin="VBAT" pad="G1"/>
<connect gate="G$1" pin="VDD" pad="D3"/>
<connect gate="G$1" pin="VDD(MID)" pad="F7"/>
<connect gate="G$1" pin="VDD(TX)" pad="E7"/>
<connect gate="G$1" pin="VEN" pad="E1"/>
<connect gate="G$1" pin="VSS(TX)" pad="G4"/>
<connect gate="G$1" pin="XTAL1" pad="A3"/>
<connect gate="G$1" pin="XTAL2" pad="C3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C1206C106J9RACTU">
<gates>
<gate name="G$1" symbol="C1206C106J9RACTU"/>
</gates>
<devices>
<device name="" package="C1206C106J9RACTU">
<connects>
<connect gate="G$1" pin="LEFT" pad="LEST"/>
<connect gate="G$1" pin="RIGHT" pad="RIGHT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XRCGB27M120F3M10R0">
<gates>
<gate name="G$1" symbol="CRYSTAL"/>
</gates>
<devices>
<device name="" package="XRCGB27M120F3M10R0">
<connects>
<connect gate="G$1" pin="L" pad="LEFT"/>
<connect gate="G$1" pin="R" pad="RIGHT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWITCH(TL3315NF160Q)">
<gates>
<gate name="G$1" symbol="SWITCH"/>
</gates>
<devices>
<device name="" package="E_BUTTON(TL3315NF160Q)">
<connects>
<connect gate="G$1" pin="A" pad="1A 2A"/>
<connect gate="G$1" pin="B" pad="3B 4B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAX17502EATB">
<description>Buck Switching Regulator IC Positive Fixed 3.3V 1 Output 1A 10-WFDFN Exposed Pad</description>
<gates>
<gate name="G$1" symbol="MAX17502"/>
</gates>
<devices>
<device name="" package="MAX175">
<connects>
<connect gate="G$1" pin="EN" pad="EN/UVLO"/>
<connect gate="G$1" pin="FB" pad="FC/VO"/>
<connect gate="G$1" pin="GND" pad="EP GND"/>
<connect gate="G$1" pin="LX" pad="LX"/>
<connect gate="G$1" pin="NC" pad="N.C/COMP"/>
<connect gate="G$1" pin="NRES" pad="NRESET"/>
<connect gate="G$1" pin="PGND" pad="PGND"/>
<connect gate="G$1" pin="SS" pad="SS"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
</connects>
<technologies>
<technology name="">
<attribute name="CURRENT_OUT" value="1A"/>
<attribute name="FREQUENCY" value="600kHz"/>
<attribute name="MSL" value="1"/>
<attribute name="VIN_MAX" value="60V"/>
<attribute name="VIN_MIN" value="4.5V"/>
<attribute name="VOUT" value="3.3"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SRR1260-150M">
<gates>
<gate name="G$1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="" package="SRR1260">
<connects>
<connect gate="G$1" pin="P1" pad="P1"/>
<connect gate="G$1" pin="P2" pad="P2"/>
</connects>
<technologies>
<technology name="">
<attribute name="INDUCTANCE" value="15uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="12PIN2.54MM">
<gates>
<gate name="G$1" symbol="12-PIN2.54MM"/>
</gates>
<devices>
<device name="" package="12PADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
