<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<text>V</text>
<text>DGC</text>
<text>Tiny
LoL
Flower</text>
<text>V</text>
<text>G</text>
<text>G</text>
</plain>
<libraries>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' Retired foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are &lt;b&gt; no longer used&lt;/b&gt; in our catalog.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ_MCU">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
<library name="LoL Clock">
<description>Generated from &lt;b&gt;LoL Clock Tunes-210_09_mini.brd&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="LOL-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
<package name="PAD_1.27X2.54_LEAF">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="L23" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L24" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L25" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L32" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L34" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L35" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L42" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L43" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L45" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L52" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L53" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="L54" library="LoL Clock" package="LOL-LED0603" value="LED_0603"/>
<element name="PAD1" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="PAD4" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="U1" library="SparkFun-Retired" package="SO08-EIAJ_MCU" value="Tiny45-20-SMT">
<attribute name="PROD_ID" value="IC-08922"/>
</element>
<element name="PAD5" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="PAD6" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="PAD2" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="PAD3" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
<element name="PAD7" library="LoL Clock" package="PAD_1.27X2.54_LEAF" value="WIREPADLEAF"/>
</elements>
<signals>
<signal name="RESET">
<contactref element="PAD5" pad="1"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="D3">
<contactref element="L23" pad="A"/>
<contactref element="L32" pad="C"/>
<contactref element="L34" pad="C"/>
<contactref element="L35" pad="C"/>
<contactref element="L43" pad="A"/>
<contactref element="L53" pad="A"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="D4">
<contactref element="L24" pad="A"/>
<contactref element="L42" pad="C"/>
<contactref element="L34" pad="A"/>
<contactref element="L43" pad="C"/>
<contactref element="L45" pad="C"/>
<contactref element="L54" pad="A"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="PAD1" pad="1"/>
<contactref element="PAD3" pad="1"/>
<contactref element="PAD7" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="U1" pad="8"/>
<contactref element="PAD4" pad="1"/>
<contactref element="PAD2" pad="1"/>
</signal>
<signal name="D0/DATA">
<contactref element="U1" pad="5"/>
<contactref element="PAD6" pad="1"/>
</signal>
<signal name="D1">
<contactref element="U1" pad="6"/>
<contactref element="L23" pad="C"/>
<contactref element="L32" pad="A"/>
<contactref element="L24" pad="C"/>
<contactref element="L42" pad="A"/>
<contactref element="L25" pad="C"/>
<contactref element="L52" pad="A"/>
</signal>
<signal name="N$1">
</signal>
<signal name="D2">
<contactref element="U1" pad="7"/>
<contactref element="L25" pad="A"/>
<contactref element="L35" pad="A"/>
<contactref element="L45" pad="A"/>
<contactref element="L52" pad="C"/>
<contactref element="L53" pad="C"/>
<contactref element="L54" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
