<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="160" y2="0" width="0" layer="20"/>
<wire x1="160" y1="0" x2="160" y2="100" width="0" layer="20"/>
<wire x1="160" y1="100" x2="0" y2="100" width="0" layer="20"/>
<wire x1="0" y1="100" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="0603-CAP">
</package>
<package name="EIA3216">
</package>
<package name="1X06">
</package>
<package name="1X02">
</package>
<package name="1X12">
</package>
<package name="0603-RES">
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="Testing">
<packages>
<package name="0603-LED-ALT1">
</package>
</packages>
</library>
<library name="burr-brown">
<description>&lt;b&gt;Burr-Brown Components&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Smal Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="switch-omron">
<description>&lt;b&gt;Omron Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SJ_2S">
<description>Small solder jumper with big paste layer so it will short during reflow.</description>
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="HC49UP">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun" package="0603-CAP" value="0.1uF"/>
<element name="C10" library="SparkFun" package="0603-CAP" value="0.1uF"/>
<element name="C13" library="SparkFun" package="EIA3216" value="10uF"/>
<element name="C19" library="SparkFun" package="EIA3216" value="10uF"/>
<element name="C2" library="SparkFun" package="0603-CAP" value="0.1uF"/>
<element name="C3" library="SparkFun" package="0603-CAP" value="0.1uF"/>
<element name="D3" library="Testing" package="0603-LED-ALT1" value="Green"/>
<element name="IC3" library="burr-brown" package="SOT223" value="REG1117">
<attribute name="MF" value=""/>
<attribute name="MPN" value="REG1117"/>
<attribute name="OC_FARNELL" value="1097566"/>
<attribute name="OC_NEWARK" value="14P6981"/>
</element>
<element name="JP1" library="SparkFun" package="1X06" value="FTDI Basic"/>
<element name="JP2" library="SparkFun" package="1X02" value=""/>
<element name="JP3" library="SparkFun" package="1X02" value=""/>
<element name="JP6" library="SparkFun" package="1X12" value=""/>
<element name="JP7" library="SparkFun" package="1X12" value=""/>
<element name="LED1" library="Testing" package="0603-LED-ALT1" value="Red"/>
<element name="R1" library="SparkFun" package="0603-RES" value=""/>
<element name="R11" library="SparkFun" package="0603-RES" value="10K"/>
<element name="R2" library="SparkFun" package="0603-RES" value="10K"/>
<element name="R3" library="SparkFun" package="0603-RES" value=""/>
<element name="R6" library="SparkFun" package="0603-RES" value="330"/>
<element name="S2" library="switch-omron" package="B3F-10XX" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="OC_NEWARK" value="36M3542"/>
</element>
<element name="SJ1" library="SparkFun-Passives" package="SJ_2S" value=""/>
<element name="U1" library="SparkFun" package="TQFP32-08" value="ATMEGA328"/>
<element name="Q1" library="crystal" package="HC49UP" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="C4" library="SparkFun" package="0603-CAP" value="0.1uF"/>
<element name="C5" library="SparkFun" package="0603-CAP" value="0.1uF"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C13" pad="C"/>
<contactref element="C10" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="D3" pad="C"/>
<contactref element="C19" pad="C"/>
<contactref element="JP7" pad="9"/>
<contactref element="JP6" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="21"/>
<contactref element="JP1" pad="5"/>
<contactref element="JP1" pad="6"/>
<contactref element="R11" pad="1"/>
<contactref element="S2" pad="3"/>
<contactref element="S2" pad="4"/>
<contactref element="IC3" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="AREF">
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="RESET">
<contactref element="JP7" pad="10"/>
<contactref element="JP6" pad="3"/>
<contactref element="U1" pad="29"/>
<contactref element="R2" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="S2" pad="2"/>
<contactref element="S2" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="JP6" pad="9"/>
<contactref element="U1" pad="17"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="JP6" pad="10"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="MOSI">
<contactref element="JP6" pad="11"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="N$7">
<contactref element="R6" pad="2"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="TXO">
<contactref element="JP7" pad="12"/>
<contactref element="U1" pad="31"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="R2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="JP6" pad="4"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
<contactref element="JP1" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="SJ1" pad="2"/>
<contactref element="C13" pad="A"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="RAW">
<contactref element="C19" pad="A"/>
<contactref element="IC3" pad="3"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="D9">
<contactref element="JP7" pad="1"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="D8">
<contactref element="JP7" pad="2"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="A5">
<contactref element="JP2" pad="2"/>
<contactref element="U1" pad="28"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="A4">
<contactref element="JP2" pad="1"/>
<contactref element="U1" pad="27"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="A3">
<contactref element="JP6" pad="5"/>
<contactref element="U1" pad="26"/>
</signal>
<signal name="A2">
<contactref element="JP6" pad="6"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="A1">
<contactref element="JP6" pad="7"/>
<contactref element="U1" pad="24"/>
</signal>
<signal name="A0">
<contactref element="JP6" pad="8"/>
<contactref element="U1" pad="23"/>
</signal>
<signal name="D2">
<contactref element="JP7" pad="8"/>
<contactref element="U1" pad="32"/>
</signal>
<signal name="D3">
<contactref element="JP7" pad="7"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="D4">
<contactref element="JP7" pad="6"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="D5">
<contactref element="JP7" pad="5"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="D6">
<contactref element="JP7" pad="4"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="D7">
<contactref element="JP7" pad="3"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="D10">
<contactref element="JP6" pad="12"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="DTR">
<contactref element="JP1" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="RXI">
<contactref element="JP1" pad="3"/>
<contactref element="JP7" pad="11"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="A6">
<contactref element="U1" pad="19"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="A7">
<contactref element="U1" pad="22"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="SJ1" pad="1"/>
<contactref element="LED1" pad="A"/>
<contactref element="IC3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R11" pad="2"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="N$5">
<contactref element="Q1" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$6">
<contactref element="Q1" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U1" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
