<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="77.9" y2="0" width="0" layer="20"/>
<wire x1="77.9" y1="0" x2="77.9" y2="37.1" width="0" layer="20"/>
<wire x1="77.9" y1="37.1" x2="0" y2="37.1" width="0" layer="20"/>
<wire x1="0" y1="37.1" x2="0" y2="0" width="0" layer="20"/>
<text>V+</text>
<text>G</text>
<text>S</text>
<text>PineApple</text>
<text>Technology</text>
<text>REV 1.0</text>
</plain>
<libraries>
<library name="switch-omron">
<description>&lt;b&gt;Omron Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B3F-40XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Sensors&lt;/h3&gt;
This library contains sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BRM-2508">
<description>&lt;h3&gt;BRM-2A18 Infrared Receiver - Horizontal Facing&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.sinoskysun.com/upload/20110512/201105120447164615.PDF"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;
&lt;li&gt;Pin Count: 3&lt;/li&gt;
&lt;li&gt;Area: 6.0 x 5.6 mm&lt;/li&gt;
&lt;li&gt;Pitch: 2.54 m,&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Devices Using:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;BRM-2A18&lt;/li&gt;
&lt;li&gt;BRM-2508&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X07">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="S1" library="switch-omron" package="B3F-40XX" value="">
<attribute name="OC_NEWARK" value="36K3105"/>
<attribute name="MPN" value="B3F-4000"/>
<attribute name="MF" value="OMRON COMPONENTS USA"/>
<attribute name="OC_FARNELL" value="176434"/>
</element>
<element name="S2" library="switch-omron" package="B3F-40XX" value="">
<attribute name="OC_NEWARK" value="36K3105"/>
<attribute name="MPN" value="B3F-4000"/>
<attribute name="MF" value="OMRON COMPONENTS USA"/>
<attribute name="OC_FARNELL" value="176434"/>
</element>
<element name="S3" library="switch-omron" package="B3F-40XX" value="">
<attribute name="OC_NEWARK" value="36K3105"/>
<attribute name="MPN" value="B3F-4000"/>
<attribute name="MF" value="OMRON COMPONENTS USA"/>
<attribute name="OC_FARNELL" value="176434"/>
</element>
<element name="S4" library="switch-omron" package="B3F-40XX" value="">
<attribute name="OC_NEWARK" value="36K3105"/>
<attribute name="MPN" value="B3F-4000"/>
<attribute name="MF" value="OMRON COMPONENTS USA"/>
<attribute name="OC_FARNELL" value="176434"/>
</element>
<element name="D1" library="SparkFun-Sensors" package="BRM-2508" value="BRM-2508RA">
<attribute name="PROD_ID" value="COMP-12059"/>
</element>
<element name="JP1" library="pinhead" package="1X07" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="S2" pad="3"/>
<contactref element="S2" pad="4"/>
<contactref element="S3" pad="3"/>
<contactref element="S3" pad="4"/>
<contactref element="S4" pad="3"/>
<contactref element="S4" pad="4"/>
<contactref element="JP1" pad="3"/>
<contactref element="D1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="S1" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="S2" pad="2"/>
<contactref element="S2" pad="1"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$7">
<contactref element="S3" pad="2"/>
<contactref element="S3" pad="1"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$8">
<contactref element="S4" pad="2"/>
<contactref element="S4" pad="1"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="VCC">
<contactref element="JP1" pad="1"/>
<contactref element="D1" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="D1" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
